|  |  |  |  |
| --- | --- | --- | --- |
| * **Classic**

[PoolTech-16](#pt16)[PoolTech-18](#PT18)[PoolTech-32](#PT32)[PoolTech-33](#PT33)[PoolTech-58](#PT58)[PoolTech-67](#PT67) | * **Overflow**

[PoolTech-88](#pt88)[PoolTech-89](#PT89)[PoolTech-99](#pt99) | * **Economy**

[PoolTech-21](#PT21) | * **Horizon**
 |
| * **Fashion Spa**

[PoolTech-08](#pt08)[PoolTech-08S](#pt08S)[PoolTech-09](#pt09)[PoolTech-09S](#pt09S)[PoolTech-12](#PT12)[PoolTech-12S](#PT12S)[PoolTech-13](#PT13) | * **Romance**

[PoolTech-61](#PT61)[PoolTech-62](#PT62)[PoolTech-62A](#PT62A)[PoolTech-63](#PT63)[PoolTech-65](#PT65)[PoolTech-66](#PT66) | * **Fish Curve**

[PoolTech-16A](#PT16A)[PoolTech-17](#PT17)[PoolTech-27](#PT27)[PoolTech-37](#PT37)[PoolTech-57](#PT57)[PoolTech-57A](#PT57A) |  |

**Følgende spa har ikke uddybende information online.** [**Kontakt**](https://pooltech.dk/kontakt/) **PoolTech for spørgsmål angående hardware, funktioner eller andet:**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| * **Classic**

[PoolTech-52](https://pooltech.dk/produkt/pooltech-52/)[PoolTech-52A](https://pooltech.dk/produkt/pooltech-52a/)[PoolTech-85](https://pooltech.dk/produkt/pooltech-85/) | * **Overflow**
 | * **Economy**

[PoolTech-28A](https://pooltech.dk/produkt/pooltech-28a/)[PoolTech-77C](https://pooltech.dk/produkt/pooltech-77c/) | * **Horizon**

|  |  |  |
| --- | --- | --- |
| [PoolTech-81](https://pooltech.dk/produkt/pooltech-81/)[PoolTech-82](https://pooltech.dk/produkt/pooltech-82/)[PoolTech-82A](https://pooltech.dk/produkt/pooltech-82a/)[PoolTech-83](https://pooltech.dk/produkt/pooltech-83/) |   |   |

 |
| * **Fashion Spa**

[PoolTech-13S](https://pooltech.dk/produkt/pooltech-13s/) | * **Romance**

[PoolTech-58B](https://pooltech.dk/produkt/pooltech-58b/) | * **Fish Curve**
 |  |

|  |  |  |  |
| --- | --- | --- | --- |
| [**PoolTech-16**](https://pooltech.dk/produkt/pooltech-16/) |   | **Electric components** |   |
|   Size |   2400x2400x930 mm |   Control System |   1 SET |
|   Seat |   6-7 Person (two louge) |   Heater |   1X3KW |
|   Material |   US Acrylic |   Whirlpool Pump |   3HPX1/2HPX2 |
|   Gross weight |   500 KG |   Circulate Pump |   1HP/0.35HPX1 |
|   Water Capacity |   1650 L |   Air Blower Pump |   400W/700WX1 |
|   |   |   |   |
| **Jets Configuration** |   | **Other Equipments** |   |
|   Total jets |   180 PCS |   Spa Top Hard Cover |   1 PCS |
|   Water therapy jets (3.5") |   10 PCS |   Insulation Foam For Shell |   1 PCS |
|   Water therapy jets (2") |   142 PCS |   Pine Wood Skirt Step |   1 SET |
|   Air bubble jets |   18 PCS |   Fountains |   2 PCS |
|   Shoulder massage jets |   2 PCS |   Ozone & Filter |   1 PCS |
|    Rotating therapy jets (5") |   1 PCS |   Underwater LED Light (5") |   1 PCS |
|   Rotating therapy jets (4") |   3 PCS |   LED Light |   34 PCS |
|   Rotating therapy jets (2.5") |   4 PCS |   Surface Valves |   1 SET |
|    |   |   Suction |   4 PCS |
|    |    |   Waterfall |   1 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
| **[PoolTech-32](https://pooltech.dk/produkt/pooltech-32/)** |   | **Electric components** |   |
|   Size |   2030x2030x920 mm |   Control System |   1 SET |
|   Seat |   7 Person  |   Heater |   1X3KW |
|   Material |   US Acrylic |   Whirlpool Pump |   3HPX1/2HPX1 |
|   Gross weight |   380 KG |   Circulate Pump |   1HP/0.35HPX1 |
|   Water Capacity |   1400 L |   Air Blower Pump |   400W/700WX1 |
|   |   |   |   |
| **Jets Configuration** |   | **Other Equipments** |   |
|   Total jets |   96 PCS |   Spa Top Hard Cover |   1 PCS |
|   Hydro therapy jets (4") |   3 PCS |   Insulation Foam For Shell |   1 PCS |
|   Hydro therapy jets (3.5") |   9 PCS |   Pine Wood Skirt Step |   1 SET |
|   Hydro therapy jets (2") |   70 PCS |   Water Fountains |   2 PCS |
|    Air jets (1.5") |   14 PCS |   Ozone & Filter |   1 PCS |
|     |    |   Underwater LED Light (5") |   1 PCS |
|    |    |   small LED Light |   12 PCS |
|    |   |   Surface Valves |   1 SET |
|    |   |   Suction |   3 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
|  **[PoolTech-33](https://pooltech.dk/produkt/pooltech-33/)**  |   | **Electric components** |  |
|   Size |   2100x1600x860 mm |   Control System |   1 SET |
|   Seat |   3 Person  |   Heater |   1X3KW |
|   Material |   US Acrylic |   Whirlpool Pump |   3HPX1 |
|   Gross weight |   290 KG |   Circulate Pump |   1HP/0.35HPX1 |
|   Water Capacity |   680 L |   Air Blower Pump |   400W/700WX1 |
|   |   |   |   |
| **Jets Configuration** |   | **Other Equipments** |   |
|   Total jets |   83 PCS |   Spa Top Hard Cover |   1 PCS |
|   Water jets (3.5") |   3 PCS |   Insulation Foam For Shell |   1 PCS |
|   Water jets (2") |   60 PCS |   Pine Wood Skirt Step |   1 SET |
|   Air jets |   20 PCS |   Water Fountains |   1 PCS |
|     |    |   Ozone & Filter |   1 PCS |
|     |    |   LED Light (5") |   1 PCS |
|    |    |   Small LED Light |   18 PCS |
|    |   |   Surface Valves |   1 SET |
|    |   |   Suction |   3 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
| **[PoolTech-58](https://pooltech.dk/produkt/pooltech-58/)** |   | **Electric components** |   |
|   Size |   2000x2000x910 mm |   Control System |   1 SET |
|   Seat |   5 Person (two louge) |   Heater |   1X3KW |
|   Material |   US Acrylic |   Whirlpool Pump |   3HPX1 |
|   Gross weight |   300 KG |   Circulate Pump |   1HP/0.35HPX1 |
|   Water Capacity |   900 L |   Air Blower Pump |   400W/700WX1 |
|   |   |   |   |
| **Jets Configuration** |   | **Other Equipments** |   |
|   Total jets |   60 PCS |   Spa Top Hard Cover |   1 PCS |
|   Single rotating jets (5") |   2 PCS |   Insulation Foam For Shell |   1 PCS |
|   Single rotating jets (3") |   2 PCS |   Pine Wood Skirt Step |   1 SET |
|   Making surf jets (5") |   1 PCS |   Water Fountains |   3 PCS |
|   Dual rotating jets (5") |   2 PCS |   Ozone & Filter |   1 PCS |
|    Water jets (5") |   3 PCS |   LED Light (5") |   1 PCS |
|   Water jets (3") |   4 PCS |   LED Light |   24 PCS |
|   Water jets (2") |   32 PCS |   Surface Valves |   1 SET |
|   Air jets |   14 PCS |   Suction |   2 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
| **[PoolTech-67](https://pooltech.dk/produkt/pooltech-67/)** |   |   Electric components |   |
|   Size |   2400x2400x950 mm |   Control System |   1 SET |
|   Seat |   6-7 Person |   Heater |   1X3KW |
|   Material |   US Acrylic |   Whirlpool Pump |   2HPX2 |
|   Gross weight |   480 KG |   Circulate Pump |   1HP/0.35HPX1 |
|   Water Capacity |   1700 L |   Air Blower Pump |   400W/700WX1 |
|   |   |   |   |
|   Jets Configuration |   |   Other Equipments |   |
|   Total jets |   65 PCS |   Spa Top Hard Cover |   1 PCS |
|   Rotating therapy jets (5") |   1 PCS |   Insulation Foam For Shell |   1 PCS |
|   Rotating therapy jets (4") |   4 PCS |   Pine Wood Skirt Step |   1 SET |
|   Water jets (4") |   10 PCS |   Water fountain |   2 PCS |
|   Water jets (2") |   32 PCS |   Ozone & Filter |   1 PCS |
|   Air jets |   18 PCS |   Underwater LED Light  |   1 PCS |
|    |    |   LED Light |   14 PCS |
|    |    |   Surface Valves |   1 SET |
|    |    |   Suction |   3 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
| **[PoolTech-18](https://pooltech.dk/produkt/pooltech-18/)** |  | **Electric components** |  |
| Size | 2400x2400x1000 mm | Control System | 1 SET |
| Seat | 6-7 Person (one louge) | Heater | 1X3KW |
| Material | US Acrylic | Whirlpool Pump | 3HPX1/2HPX2 |
| Gross weight | 500 KG | Circulate Pump | 1HP/0.35HPX1 |
| Water Capacity | 1690 L | Air Blower Pump | 400W/700WX1 |
|  |  |  |  |
| **Jets Configuration** |  | **Other Equipments** |  |
| Total jets | 126 PCS | Spa Top Hard Cover | 1 PCS |
| Water therapy jets (2.5") | 33 PCS | Insulation Foam For Shell | 1 PCS |
| Water jets (2") | 73 PCS | Pine Wood Skirt Step | 1 SET |
| Air jets | 16 PCS | Fountains | 2 PCS |
| Surfing jets (5") | 1 PCS | Ozone & Filter | 1 PCS |
| Rotating therapy jets (5") | 3 PCS | Underwater LED Light (5") | 1 PCS |
|  |  | LED Light | 15 PCS |
|  |  | Surface Valves | 1 SET |
|  |  | Suction | 4 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
| **[PoolTech-88](https://pooltech.dk/produkt/pooltech-88/)**  |  | **Electric components** |  |
|   Size |   2400x2400x930 mm |   Control System |   1 SET |
|   Seat |   7-8 Person |   Heater |   1X3KW |
|   Material |   US Acrylic |   Whirlpool Pump |   3HPX1/2HPX1 |
|   Gross weight |   480 KG |   Circulate Pump |   0.35HPX2 |
|   Water Capacity |   600 L |   Air Blower Pump |   400W/700WX1 |
|   |   |   |   |
|   Jets Configuration |   |   Other Equipments |   |
|   Total jets |   89 PCS |   Spa Top Hard Cover |   1 PCS |
|   Surfing jet (5") |   1 PCS |   Insulation Foam For Shell |   1 PCS |
|   Rotating therapy jets (5") |   2 PCS |   Pine Wood Skirt Step |   1 SET |
|   Rotating therapy jets (3.5") |   9 PCS |    |    |
|   Water jets (5") |   2 PCS |   Ozone & Filter |   1 PCS |
|   Water jets (3.5") |   10 PCS |   Underwater LED Light  |   1 PCS |
|   Water jets (2") |   51 PCS |   LED Light |   12 PCS |
|   Air jets |   14 PCS |   Surface Valves |   1 SET |
|    |    |   Suction |   3 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
|  [**PoolTech-89**](https://pooltech.dk/produkt/pooltech-89/) |   | **Electric components** |  |
|   Size |   2400x2400x930 mm |   Control System |   1 SET |
|   Seat |   6-7 Person |   Heater |   1X3KW |
|   Material |   US Acrylic |   Whirlpool Pump |   3HPX1/2HPX1 |
|   Gross weight |   480 KG |   Circulate Pump |   0.35HPX2 |
|   Water Capacity |   600 L |   Air Blower Pump |   400W/700WX1 |
|   |   |   |   |
| **Jets Configuration** |   | **Other Equipments** |   |
|   Total jets |   79 PCS |   Spa Top Hard Cover |   1 PCS |
|   Surfing jet (5") |   1 PCS |   Insulation Foam For Shell |   1 PCS |
|   Rotating therapy jets (3.5") |   5 PCS |   Pine Wood Skirt Step |   1 SET |
|   Water jets (5") |   2 PCS |    |    |
|   Water jets (3.5") |   10 PCS |   Ozone & Filter |   1 PCS |
|   Water jets (2") |   45 PCS |   Underwater LED Light  |   1 PCS |
|   Air jets |   16 PCS |   LED Light |   12 PCS |
|    |    |   Surface Valves |   1 SET |
|    |    |   Suction |   4 PCS |
| **[PoolTech-99](https://pooltech.dk/produkt/pooltech-99/)** |   |   **Electric components** |   |
|   Size |   3800x2400x930 mm |   Control System |   1 SET |
|   Seat |   13-14 Person |   Heater |   1X3KW |
|   Material |   US Acrylic |   Whirlpool Pump |   3HPX1/2HPX2 |
|   Gross weight |   1100 KG |   Circulate Pump |   0.35HPX2 |
|   Water Capacity |   4300 L |   Air Blower Pump |   400W/700WX1 |
|   |   |   |   |
|   **Jets Configuration** |   |   **Other Equipments** |   |
|   Total jets |   119 PCS |   Spa Top Hard Cover |   1 PCS |
|   Rotating therapy jets (3.5") |   10 PCS |   Insulation Foam For Shell |   1 PCS |
|   Water jets (5") |   2 PCS |   Pine Wood Skirt Step |   1 SET |
|   Water jets (3.5") |   12 PCS |    |    |
|   Water jets (2") |   69 PCS |   Ozone & Filter |   1 PCS |
|   Air jets |   26 PCS |   Underwater LED Light  |   2 PCS |
|   |    |   LED Light |   16 PCS |
|    |    |   Surface Valves |   1 SET |
|    |    |   Suction |   4 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
| **[PoolTech-08](https://pooltech.dk/produkt/pooltech-08/)** |  | **Electric components** |  |
| Size | 2400x2400x930 mm | Control System | 1 SET |
| Seat | 6-7 Person (two louge) | Heater | 1X3KW |
| Material | US Acrylic | Whirlpool Pump | 3HPX1/2HPX1 |
| Gross weight | 500 KG | Circulate Pump | 1HP/0.35HPX1 |
| Water Capacity | 1650 L | Air Blower Pump | 400W/700WX1 |
|  |  |  |  |
| **Jets Configuration** |  | **Other Equipments** |  |
| Total jets | 102 PCS | Spa Top Hard Cover | 1 PCS |
| Water therapy jets (5") | 1 PCS | Insulation Foam For Shell | 1 PCS |
| Water therapy jets (3.5") | 7 PCS | Pine Wood Skirt Step | 1 SET |
| Water therapy jets (2") | 73 PCS | Waterfall | 1 PCS |
| air jets | 14 PCS | Ozone & Filter | 1 PCS |
| Rotating therapy jets (3.5") | 7 PCS | LED Light (5") | 1 PCS |
|  |  | LED Light (Small) | 45 PCS |
|  |  | Surface Valves | 1 SET |
|  |  | Suction | 3 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
| **[PoolTech-08S](https://pooltech.dk/produkt/pooltech-08s/)** |   | **Electric components** |   |
|   Size |   2200x2200x970 mm |   Control System |   1 SET |
|   Seat |   6 Person (one louge) |   Heater |   1X3KW |
|   Material |   US Acrylic |   Whirlpool Pump |   2HPX2 |
|   Gross weight |   360 KG |   Circulate Pump |   0.35HPX1 |
|   Water Capacity |   1400 L |   Air Blower Pump |   / |
|   |   |   |   |
| **Jets Configuration** |   | **Other Equipments** |   |
|   Total jets |   76 PCS |   Spa Top Hard Cover |   1 PCS |
|   Water therapy jets (5") |   1 PCS |   Insulation Foam For Shell |   1 PCS |
|   Water therapy jets (3.5") |   11 PCS |   Pine Wood Skirt Step |   1 SET |
|   Water therapy jets (2") |   58 PCS |   Waterfall |   1 PCS |
|   Rotating jets (3.5") |   6 PCS |   Ozone & Filter |   1 PCS |
|     |    |   LED Light (5") |   1 PCS |
|   |    |   LED Light (Small) |   31 PCS |
|    |    |   Surface Valves |   1 SET |
|    |   |   Suction |   3 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
| **[PoolTech-09](https://pooltech.dk/produkt/pooltech-09/)** |   | **Electric components** |   |
|   Size |   2200x2200x970 mm |   Control System |   1 SET |
|   Seat |   7 Person (one louge) |   Heater |   1X3KW |
|   Material |   US Acrylic |   Whirlpool Pump |   3HPX1/2HPX1 |
|   Gross weight |   400 KG |   Circulate Pump |   0.35HPX1 |
|   Water Capacity |   1400 L |   Air Blower Pump |   400WX1 |
|   |   |   |   |
| **Jets Configuration** |   | **Other Equipments** |   |
|   Total jets |   109 PCS |   Spa Top Hard Cover |   1 PCS |
|   Water therapy jets (5") |   2 PCS |   Insulation Foam For Shell |   1 PCS |
|   Water therapy jets (3.5") |   5 PCS |   Pine Wood Skirt Step |   1 SET |
|   Water jets (2") |   83 PCS |   Fountain |   2 PCS |
|   air jets |   14 PCS |   Ozone & Filter |   1 PCS |
|    Water Rotating jets (3.5") |   4 PCS |   LED Light (5") |   1 PCS |
|   |    |   LED Light (Small) |   48 PCS |
|    |    |   Surface Valves |   1 SET |
|    |   |   Suction |   3 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
| **[PoolTech-09S](https://pooltech.dk/produkt/pooltech-09s/)** |   | **Electric components** |   |
|   Size |   2200x2200x970 mm |   Control System |   1 SET |
|   Seat |   7 Person (one louge) |   Heater |   1X3KW |
|   Material |   US Acrylic |   Whirlpool Pump |   2HPX2 |
|   Gross weight |   360 KG |   Circulate Pump |   0.35HPX1 |
|   Water Capacity |   1400 L |   Air Blower Pump |   / |
|   |   |   |   |
| **Jets Configuration** |   | **Other Equipments** |   |
|   Total jets |   68 PCS |   Spa Top Hard Cover |   1 PCS |
|   Water therapy jets (5") |   3 PCS |   Insulation Foam For Shell |   1 PCS |
|   Water therapy jets (3.5") |   9 PCS |   Pine Wood Skirt Step |   1 SET |
|   Water therapy jets (2") |   50 PCS |   Fountain |   1 PCS |
|   Rotating jets (3.5") |   6 PCS |   Ozone & Filter |   1 PCS |
|     |   |   LED Light (5") |   1 PCS |
|   |    |   LED Light (Small) |   34 PCS |
|    |    |   Surface Valves |   1 SET |
|    |   |   Suction |   3 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
| **[PoolTech-12](https://pooltech.dk/produkt/pooltech-12/)** |  | **Electric components** |  |
| Size | 2200x2200x970 mm | Control System | 1 SET |
| Seat | 5 Person | Heater | 1X3KW |
| Material | US Acrylic | Whirlpool Pump | 3HPX1/2HPX1 |
| Gross weight | 400 KG | Circulate Pump | 1HP/0.35HPX1 |
| Water Capacity | 1400 L | Air Blower Pump | 400W/700WX1 |
|  |  |  |  |
| **Jets Configuration** |  | **Other Equipments** |  |
| Total jets | 102 PCS | Spa Top Hard Cover | 1 PCS |
| Water therapy jets (5") | 3 PCS | Insulation Foam For Shell | 1 PCS |
| Water therapy jets (3.5") | 10 PCS | Pine Wood Skirt Step | 1 SET |
| Water therapy jets (2") | 49 PCS | Fountain | 1 PCS |
| Rotating therapy jets (3.5") | 8 PCS | Ozone & Filter | 1 PCS |
|  |  | LED Light (5") | 1 PCS |
|  |  | LED Light (Small) | 42 PCS |
|  |  | Surface Valves | 1 SET |
|  |  | Suction | 3 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
| **[PoolTech-12S](https://pooltech.dk/produkt/pooltech-12s/)** |   | **Electric components** |   |
|   Size |   2200x2200x970 mm |   Control System |   1 SET |
|   Seat |   5 Person |   Heater |   1X3KW |
|   Material |   US Acrylic |   Whirlpool Pump |   2HPX2 |
|   Gross weight |   400 KG |   Circulate Pump |   0.35HPX1 |
|   Water Capacity |   1400 L |   Air Blower Pump |   / |
|   |   |   |   |
| **Jets Configuration** |   | **Other Equipments** |   |
|   Total jets |   70 PCS |   Spa Top Hard Cover |   1 PCS |
|   Water therapy jets (5") |   3 PCS |   Insulation Foam For Shell |   1 PCS |
|   Water therapy jets (3.5") |   10 PCS |   Pine Wood Skirt Step |   1 SET |
|   Water therapy jets (2") |   49 PCS |   Fountain |   3 PCS |
|   Rotating jets (3.5") |   8 PCS |   Ozone & Filter |   1 PCS |
|     |   |   LED Light (5") |   1 PCS |
|   |    |   LED Light (Small) |   42 PCS |
|    |    |   Surface Valves |   1 SET |
|    |   |   Suction |   3 PCS |
|    |    |   Waterfall |   1 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
| **[PoolTech-13](https://pooltech.dk/produkt/pooltech-13/)** |   | **Electric components** |   |
|   Size |   2100x1500x820 mm |   Control System |   1 SET |
|   Seat |   3 Person |   Heater |   1X3KW |
|   Material |   US Acrylic |   Whirlpool Pump |   3HPX1 |
|   Gross weight |   250 KG |   Circulate Pump |   0.35HPX1 |
|   Water Capacity |   650 L |   Air Blower Pump |   400WX1 |
|   |   |   |   |
| **Jets Configuration** |   | **Other Equipments** |   |
|   Total jets |   39 PCS |   Spa Top Hard Cover |   1 PCS |
|   Water therapy jets (5") |   1 PCS |   Insulation Foam For Shell |   1 PCS |
|   Water therapy jets (3.5") |   2 PCS |   Pine Wood Skirt Step |   1 SET |
|   Water therapy jets (2") |   24 PCS |   Waterfall |   1 PCS |
|   Roating therapy Jets (3.5") |   2 PCS |   Ozone & Filter |   1 PCS |
|   Air jets |   10 PCS |   LED Light (5") |   1 PCS |
|    |   |   LED Light (Small) |   31 PCS |
|    |    |   Surface Valves |   1 SET |
|    |   |   Suction |   2 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
| **[PoolTech-61](https://pooltech.dk/produkt/pooltech-61/)** |   | **Electric components** |   |
|   Size |   2100x1700x870 mm |   Control System |   1 SET |
|   Seat |   3 Person |   Heater |   1X3KW |
|   Material |   US Acrylic |   Whirlpool Pump |   3HPX1 |
|   Gross weight |   300 KG |   Circulate Pump |   1HP/0.35HPX1 |
|   Water Capacity |   600 L |   Air Blower Pump |   400W/700WX1 |
|   |   |   |   |
| **Jets Configuration** |   | **Other Equipments** |   |
|   Total jets |   41 PCS |   Spa Top Hard Cover |   1 PCS |
|   Rotating therapy jets (5") |   1 PCS |   Insulation Foam For Shell |   1 PCS |
|   Rotating therapy jets (4.5") |   2 PCS |   Pine Wood Skirt Step |   1 SET |
|   Rotating therapy jets (3.5") |   4 PCS |   Waterfall |   1 PCS |
|   Water jets (3.5") |   10 PCS |   Ozone & Filter |   1 PCS |
|   Water jets (2.5") |   17 PCS |   LED Light (5") |   1 PCS |
|   Air jets |   6 PCS |   LED Light |   16 PCS |
|    |   |   Surface Valves |   1 SET |
|   |   |   Suction |   2 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
| **[PoolTech-62](https://pooltech.dk/produkt/pooltech-62/)** |   | **Electric components** |   |
|   Size |   2200x2200x930 mm |   Control System |   1 SET |
|   Seat |   5 Person (one louge) |   Heater |   1X3KW |
|   Material |   US Acrylic |   Whirlpool Pump |   3HPX1/2HPX1 |
|   Gross weight |   400 KG |   Circulate Pump |   1HP/0.35HPX1 |
|   Water Capacity |   1340 L |   Air Blower Pump |   400W/700WX1 |
|   |   |   |   |
| **Jets Configuration** |   | **Other Equipments** |   |
|   Total jets |   57 PCS |   Spa Top Hard Cover |   1 PCS |
|   Big Surfing jets (8") |   1 PCS |   Insulation Foam For Shell |   1 PCS |
|   Rotating therapy jets (5") |   1 PCS |   Pine Wood Skirt Step |   1 SET |
|   Rotating therapy jets (4.5") |   6 PCS |   Fountains |   / |
|   Water jets (5") |   2 PCS |   Ozone & Filter |   1 PCS |
|   Water jets (4.5") |   2 PCS |   Underwater LED Light (5") |   1 PCS |
|   Water jets (3.5") |   19 PCS |   LED Light |   28 PCS |
|   Water jets (2.5")  |   12 PCS |   Surface Valves |   1 SET |
|   Water jets (2") |   2 PCS |   Suction |   3 PCS |
|   Air jets |   10 PCS |   Waterfall |   1 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
| **[PoolTech-62A](https://pooltech.dk/produkt/pooltech-62a/)** |   | **Electric components** |   |
|   Size |   2200x2200x930 mm |   Control System |   1 SET |
|   Seat |   5 Person (one louge) |   Heater |   1X3KW |
|   Material |   US Acrylic |   Whirlpool Pump |   3HPX11 |
|   Gross weight |   400 KG |   Circulate Pump |   1HP/0.35HPX1 |
|   Water Capacity |   1340 L |   Air Blower Pump |   400W/700WX1 |
|   |   |   |   |
| **Jets Configuration** |   | **Other Equipments** |   |
|   Total jets |   42 PCS |   Spa Top Hard Cover |   1 PCS |
|   Rotating therapy jets (5") |   1 PCS |   Insulation Foam For Shell |   1 PCS |
|   Rotating therapy jets (3.5") |   2 PCS |   Pine Wood Skirt Step |   1 SET |
|   Water jets (4.5") |   9 PCS |   Fountains |   / |
|   Water jets (3.5") |   9 PCS |   Ozone & Filter |   1 PCS |
|   Water jets (2.5") |   11 PCS |   Underwater LED Light (5") |   1 PCS |
|   Air jets |   10 PCS |   LED Light |   21 PCS |
|    |    |   Surface Valves |   1 SET |
|   |    |   Suction |   2 PCS |
|   |    |   Waterfall |   1 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
| [**PoolTech-63**](https://pooltech.dk/produkt/pooltech-63/) |   | **Electric components** |   |
|   Size |   2200x2200x930 mm |   Control System |   1 SET |
|   Seat |   6 Person (one louge) |   Heater |   1X3KW |
|   Material |   US Acrylic |   Whirlpool Pump |   3HPX1/2HPX1 |
|   Gross weight |   400 KG |   Circulate Pump |   1HP/0.35HPX1 |
|   Water Capacity |   1380 L |   Air Blower Pump |   400W/700WX1 |
|   |   |   |   |
| **Jets Configuration** |   | **Other Equipments** |   |
|   Total jets |   60 PCS |   Spa Top Hard Cover |   1 PCS |
|   Big Surfing jets (8") |   1 PCS |   Insulation Foam For Shell |   1 PCS |
|   Rotating therapy jets (4.5") |   4 PCS |   Pine Wood Skirt Step |   1 SET |
|   Rotating therapy jets (3.5") |   2 PCS |   Waterfall |   2 PCS |
|   Water jets (5") |   2 PCS |   Ozone & Filter |   1 PCS |
|   Water jets (4.5") |   8 PCS |   Underwater LED Light (5") |   1 PCS |
|   Water jets (3.5") |   11 PCS |   LED Light |   21 PCS |
|   Water jets (2.5")  |   20 PCS |   Surface Valves |   1 SET |
|   Air jets |   12 PCS |   Suction |   3 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
| [**PoolTech-65**](https://pooltech.dk/produkt/pooltech-65/) |   | **Electric components** |   |
|   Size |   2300x2300x930 mm |   Control System |   1 SET |
|   Seat |   5 Person (two louge) |   Heater |   1X3KW |
|   Material |   US Acrylic |   Whirlpool Pump |   3HPX2/2HPX1 |
|   Gross weight |   450 KG |   Circulate Pump |   1HP/0.35HPX1 |
|   Water Capacity |   1450 L |   Air Blower Pump |   400W/700WX1 |
|   |   |   |   |
| **Jets Configuration** |   | **Other Equipments** |   |
|   Total jets |   106 PCS |   Spa Top Hard Cover |   1 PCS |
|   Rotating therapy jets (5") |   6 PCS |   Insulation Foam For Shell |   1 PCS |
|   Rotating therapy jets (2.5") |   4 PCS |   Pine Wood Skirt Step |   1 SET |
|   Water jets (5") |   2 PCS |   Waterfall |   1 PCS |
|   Water jets (4") |   8 PCS |   Ozone & Filter |   1 PCS |
|   Water jets (3.5") |   33 PCS |   Underwater LED Light (5") |   1 PCS |
|   Water jets (2.5") |   2 PCS |   LED Light |   19 PCS |
|   Water jets (2") |   37 PCS |   Surface Valves |   1 SET |
|  Air jets |   14 PCS |   Suction |   4 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
| **[PoolTech-66](https://pooltech.dk/produkt/pooltech-66/)** |   | **Electric components** |   |
|   Size |   2400x2400x930 mm |   Control System |   1 SET |
|   Seat |   6-7 Person (two louge) |   Heater |   1X3KW |
|   Material |   US Acrylic |   Whirlpool Pump |   3HPX2/2HPX1 |
|   Gross weight |   500 KG |   Circulate Pump |   1HP/0.35HPX1 |
|   Water Capacity |   1650 L |   Air Blower Pump |   400W/700WX1 |
|   |   |   |   |
| **Jets Configuration** |   | **Other Equipments** |   |
|   Total jets |   123 PCS |   Spa Top Hard Cover |   1 PCS |
|   Large surfing jets (7") |   3 PCS |   Insulation Foam For Shell |   1 PCS |
|   Rotating therapy jets (5") |   2 PCS |   Pine Wood Skirt Step |   1 SET |
|   Rotating therapy jets (4") |   6 PCS |   Water fountain |   3 PCS |
|   Rotating therapy jets (2.5") |   2 PCS |   Ozone & Filter |   1 PCS |
|   Water jets (4") |   13 PCS |   Underwater LED Light  |   1 PCS |
|   Water jets (3") |   4 PCS |   LED Light |   30 PCS |
|   Water jets (2.5") |   39 PCS |   Surface Valves |   1 SET |
|   Water jets (2") |   40 PCS |   Suction |   5 PCS |
|   Air jets |   14 PCS |   |    |

|  |  |  |  |
| --- | --- | --- | --- |
| **[PoolTech-21](https://pooltech.dk/produkt/pooltech-21/)** |   | **Electric components** |   |
|   Size |   1800x1300x840 mm |   Control System |   1 SET |
|   Seat |   2-3 Person |   Heater |   1X3KW |
|   Material |   US Acrylic |   Whirlpool Pump |   2HPX1 |
|   Gross weight |   260 KG |   Circulate Pump |   1HP/0.35HPX1 |
|   Water Capacity |   510 L |   Air Blower Pump |   400W/700WX1 |
|   |   |   |   |
| **Jets Configuration** |   | **Other Equipments** |   |
|   Total jets |   39 PCS |   Spa Top Hard Cover |   1 PCS |
|   Hydro therapy water jets (2.5") |   15 PCS |   Insulation Foam For Shell |   1 PCS |
|   Water jets (2") |   13 PCS |   Pine Wood Skirt Step |   1 SET |
|   Air jets |   11 PCS |   Drainage |   1 PCS |
|    |   |   Ozone & Filter |   1 PCS |
|   |   |   LED Light (5") |   1 PCS |
|   |    |    LED Light (2") |   8 PCS |
|   |    |   Surface Valves |   1 SET |
|    |   |   Suction |   1 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
| **[PoolTech-16A](https://pooltech.dk/produkt/pooltech-16a/)** |   | **Electric components** |   |
|   Size |   2400x2400x930 mm |   Control System |   1 SET |
|   Seat |   6-7 Person (two louge) |   Heater |   1X3KW |
|   Material |   US Acrylic |   Whirlpool Pump |   3HPX1/2HPX2 |
|   Gross weight |   500 KG |   Circulate Pump |   1HP/0.35HPX1 |
|   Water Capacity |   1650 L |   Air Blower Pump |   400W/700WX1 |
|   |   |   |   |
| **Jets Configuration** |   | **Other Equipments** |   |
|   Total jets |   163 PCS |   Spa Top Hard Cover |   1 PCS |
|   Water jets (5") |   2 PCS |   Insulation Foam For Shell |   1 PCS |
|   Water jets (4") |   7 PCS |   Pine Wood Skirt Step |   1 SET |
|   Water jets (3") |   6 PCS |   Fountains |   2 PCS |
|   Water jets (2") |   115 PCS |   Ozone & Filter |   1 PCS |
|    Rotating therapy jets (3") |   8 PCS |   Underwater LED Light (5") |   1 PCS |
|   Surfing jets (5") |   1 PCS |   LED Light |   20 PCS |
|   Air jets |   22 PCS |   Surface Valves |   1 SET |
|   Shoulder massage jets |   2 PCS |   Suction |   5 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
| **[PoolTech-17](https://pooltech.dk/produkt/pooltech-17/)** |   | **Electric components** |   |
|   Size |   2200x2200x930 mm |   Control System |   1 SET |
|   Seat |   5 Person (two louge) |   Heater |   1X3KW |
|   Material |   US Acrylic |   Whirlpool Pump |   3HPX1/2HPX1 |
|   Gross weight |   390 KG |   Circulate Pump |   1HP/0.35HPX1 |
|   Water Capacity |   1600 L |   Air Blower Pump |   400W/700WX1 |
|   |   |   |   |
| **Jets Configuration** |   | **Other Equipments** |   |
|   Total jets |   67 PCS |   Spa Top Hard Cover |   1 PCS |
|   Water jets (3.5") |   16 PCS |   Insulation Foam For Shell |   1 PCS |
|   Water jets (2") |   32 PCS |   Pine Wood Skirt Step |   1 SET |
|   Air jets |   12 PCS |   Fountains |   1 PCS |
|   Surfing jets (5") |   1 PCS |   Ozone & Filter |   1 PCS |
|    Rotating therapy jets (5") |   2 PCS |   Underwater LED Light  |   1 PCS |
|   Rotating therapy jets (4") |   4 PCS |   LED Light |   15 PCS |
|    |   |   Surface Valves |   1 SET |
|    |   |   Suction |   4 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
| **[PoolTech-27](https://pooltech.dk/produkt/pooltech-27/)** |   | **Electric components** |   |
|   Size |   2100x1600x870 mm |   Control System |   1 SET |
|   Seat |   3 Person (two louge) |   Heater |   1X3KW |
|   Material |   US Acrylic |   Whirlpool Pump |   3HPX1 |
|   Gross weight |   300 KG |   Circulate Pump |   1HP/0.35HPX1 |
|   Water Capacity |   600 L |   Air Blower Pump |   400W/700WX1 |
|   |   |   |   |
| **Jets Configuration** |   | **Other Equipments** |   |
|   Total jets |   40 PCS |   Spa Top Hard Cover |   1 PCS |
|   Water jets (5") |   2 PCS |   Insulation Foam For Shell |   1 PCS |
|   Water jets (2") |   16 PCS |   Pine Wood Skirt Step |   1 SET |
|   Air jets |   8 PCS |   Fountains |   / |
|   Rotating therapy jets (4") |   4 PCS |   Ozone & Filter |   1 PCS |
|   Hydrotherapy jets (3.5") |   10 PCS |   LED Light (5") |   1 PCS |
|   |    |   LED Light |   13 PCS |
|   |    |   Surface Valves |   1 SET |
|    |   |   Suction |   3 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
| **[PoolTech-37](https://pooltech.dk/produkt/pooltech-37/)** |   | **Electric components** |   |
|   Size |   2200x2200x930 mm |   Control System |   1 SET |
|   Seat |   5 Person  |   Heater |   1X3KW |
|   Material |   US Acrylic |   Whirlpool Pump |   3HPX1 |
|   Gross weight |   410 KG |   Circulate Pump |   1HP/0.35HPX1 |
|   Water Capacity |   1350 L |   Air Blower Pump |   400W/700WX1 |
|   |   |   |   |
| **Jets Configuration** |   | **Other Equipments** |   |
|   Total jets |   72 PCS |   Spa Top Hard Cover |   1 PCS |
|   Water jets (5") |   1 PCS |   Insulation Foam For Shell |   1 PCS |
|   Water jets (4") |   8 PCS |   Pine Wood Skirt Step |   1 SET |
|   Air jets  |   16 PCS |   Water Fountains |   2 PCS |
|   Water jets (2") |   33 PCS |   Ozone & Filter |   1 PCS |
|   Rotating therapy jets (4") |   8 PCS |   LED Light (5") |   1 PCS |
|  Rotating therapy jets (2.5") |   6 PCS |   LED Light |   18 PCS |
|    |   |   Surface Valves |   1 SET |
|    |   |   Suction |   3 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
| **[PoolTech-57](https://pooltech.dk/produkt/pooltech-57/)** |   | **Electric components** |   |
|   Size |   1950x1950x930 mm |   Control System |   1 SET |
|   Seat |   4-6 Person |   Heater |   1X3KW |
|   Material |   US Acrylic |   Whirlpool Pump |   3HPX1 |
|   Gross weight |   280 KG |   Circulate Pump |   1HP/0.35HPX1 |
|   Water Capacity |   900 L |   Air Blower Pump |   400W/700WX1 |
|   |   |   |   |
| **Jets Configuration** |   | **Other Equipments** |   |
|   Total jets |   36 PCS |   Spa Top Hard Cover |   1 PCS |
|   Rotating therapy jets (5") |   1 PCS |   Insulation Foam For Shell |   1 PCS |
|   Rotating therapy jets (4") |   2 PCS |   Pine Wood Skirt Step |   1 SET |
|   Water jets (4") |   6 PCS |   Fountains |   2 PCS |
|   Water jets (3.5") |   2 PCS |   Ozone & Filter |   1 PCS |
|    Water jets (2") |   17 PCS |   LED Light (5") |   1 PCS |
|   Air jets |   8 PCS |   LED Light |   15 PCS |
|    |    |   Surface Valves |   1 SET |
|    |   |   Suction |   3 PCS |
|    |    |   Waterfall |   1 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
| **[PoolTech-57A](https://pooltech.dk/produkt/pooltech-57a/)** |   | **Electric components** |   |
|   Size |   1950x1950x930 mm |   Control System |   1 SET |
|   Seat |   5 Person (one louge) |   Heater |   1X3KW |
|   Material |   US Acrylic |   Whirlpool Pump |   3HPX1 |
|   Gross weight |   290 KG |   Circulate Pump |   1HP/0.35HPX1 |
|   Water Capacity |   950 L |   Air Blower Pump |   400W/700WX1 |
|   |   |   |   |
| **Jets Configuration** |   | **Other Equipments** |   |
|   Total jets |   40 PCS |   Spa Top Hard Cover |   1 PCS |
|   Surfing therapy jets (5") |   1 PCS |   Insulation Foam For Shell |   1 PCS |
|   Hydro therapy jets (5") |   2 PCS |   Pine Wood Skirt Step |   1 SET |
|   Hydro therapy jets (4") |   1 PCS |   Fountains |   2 PCS |
|   Hydro therapy jets (3.5") |   8 PCS |   Ozone & Filter |   1 PCS |
|    Hydro therapy jets (2") |   20 PCS |   LED Light (5") |   1 PCS |
|   Air jets (1.5") |   8 PCS |   LED Light |   18 PCS |
|    |    |   Surface Valves |   1 SET |
|    |   |   Suction |   2 PCS |