|  |  |  |  |
| --- | --- | --- | --- |
| * **Classic**   [PoolTech-16](#pt16) [PoolTech-18](#PT18)  [PoolTech-32](#PT32)  [PoolTech-33](#PT33)  [PoolTech-58](#PT58)  [PoolTech-67](#PT67) | * **Overflow**   [PoolTech-88](#pt88)  [PoolTech-89](#PT89)  [PoolTech-99](#pt99) | * **Economy**   [PoolTech-21](#PT21) | * **Horizon** |
| * **Fashion Spa**   [PoolTech-08](#pt08)  [PoolTech-08S](#pt08S)  [PoolTech-09](#pt09)  [PoolTech-09S](#pt09S)  [PoolTech-12](#PT12)  [PoolTech-12S](#PT12S)  [PoolTech-13](#PT13) | * **Romance**   [PoolTech-61](#PT61)  [PoolTech-62](#PT62)  [PoolTech-62A](#PT62A)  [PoolTech-63](#PT63)  [PoolTech-65](#PT65)  [PoolTech-66](#PT66) | * **Fish Curve**   [PoolTech-16A](#PT16A)  [PoolTech-17](#PT17)  [PoolTech-27](#PT27)  [PoolTech-37](#PT37)  [PoolTech-57](#PT57)  [PoolTech-57A](#PT57A) |  |

**Følgende spa har ikke uddybende information online.** [**Kontakt**](https://pooltech.dk/kontakt/) **PoolTech for spørgsmål angående hardware, funktioner eller andet:**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| * **Classic**   [PoolTech-52](https://pooltech.dk/produkt/pooltech-52/)  [PoolTech-52A](https://pooltech.dk/produkt/pooltech-52a/)  [PoolTech-85](https://pooltech.dk/produkt/pooltech-85/) | * **Overflow** | * **Economy**   [PoolTech-28A](https://pooltech.dk/produkt/pooltech-28a/)  [PoolTech-77C](https://pooltech.dk/produkt/pooltech-77c/) | * **Horizon**  |  |  |  | | --- | --- | --- | | [PoolTech-81](https://pooltech.dk/produkt/pooltech-81/) [PoolTech-82](https://pooltech.dk/produkt/pooltech-82/) [PoolTech-82A](https://pooltech.dk/produkt/pooltech-82a/) [PoolTech-83](https://pooltech.dk/produkt/pooltech-83/) |  |  | |
| * **Fashion Spa**   [PoolTech-13S](https://pooltech.dk/produkt/pooltech-13s/) | * **Romance**   [PoolTech-58B](https://pooltech.dk/produkt/pooltech-58b/) | * **Fish Curve** |  |

|  |  |  |  |
| --- | --- | --- | --- |
| [**PoolTech-16**](https://pooltech.dk/produkt/pooltech-16/) |  | **Electric components** |  |
| Size | 2400x2400x930 mm | Control System | 1 SET |
| Seat | 6-7 Person (two louge) | Heater | 1X3KW |
| Material | US Acrylic | Whirlpool Pump | 3HPX1/2HPX2 |
| Gross weight | 500 KG | Circulate Pump | 1HP/0.35HPX1 |
| Water Capacity | 1650 L | Air Blower Pump | 400W/700WX1 |
|  |  |  |  |
| **Jets Configuration** |  | **Other Equipments** |  |
| Total jets | 180 PCS | Spa Top Hard Cover | 1 PCS |
| Water therapy jets (3.5") | 10 PCS | Insulation Foam For Shell | 1 PCS |
| Water therapy jets (2") | 142 PCS | Pine Wood Skirt Step | 1 SET |
| Air bubble jets | 18 PCS | Fountains | 2 PCS |
| Shoulder massage jets | 2 PCS | Ozone & Filter | 1 PCS |
| Rotating therapy jets (5") | 1 PCS | Underwater LED Light (5") | 1 PCS |
| Rotating therapy jets (4") | 3 PCS | LED Light | 34 PCS |
| Rotating therapy jets (2.5") | 4 PCS | Surface Valves | 1 SET |
|  |  | Suction | 4 PCS |
|  |  | Waterfall | 1 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
| **[PoolTech-32](https://pooltech.dk/produkt/pooltech-32/)** |  | **Electric components** |  |
| Size | 2030x2030x920 mm | Control System | 1 SET |
| Seat | 7 Person | Heater | 1X3KW |
| Material | US Acrylic | Whirlpool Pump | 3HPX1/2HPX1 |
| Gross weight | 380 KG | Circulate Pump | 1HP/0.35HPX1 |
| Water Capacity | 1400 L | Air Blower Pump | 400W/700WX1 |
|  |  |  |  |
| **Jets Configuration** |  | **Other Equipments** |  |
| Total jets | 96 PCS | Spa Top Hard Cover | 1 PCS |
| Hydro therapy jets (4") | 3 PCS | Insulation Foam For Shell | 1 PCS |
| Hydro therapy jets (3.5") | 9 PCS | Pine Wood Skirt Step | 1 SET |
| Hydro therapy jets (2") | 70 PCS | Water Fountains | 2 PCS |
| Air jets (1.5") | 14 PCS | Ozone & Filter | 1 PCS |
|  |  | Underwater LED Light (5") | 1 PCS |
|  |  | small LED Light | 12 PCS |
|  |  | Surface Valves | 1 SET |
|  |  | Suction | 3 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
| **[PoolTech-33](https://pooltech.dk/produkt/pooltech-33/)** |  | **Electric components** |  |
| Size | 2100x1600x860 mm | Control System | 1 SET |
| Seat | 3 Person | Heater | 1X3KW |
| Material | US Acrylic | Whirlpool Pump | 3HPX1 |
| Gross weight | 290 KG | Circulate Pump | 1HP/0.35HPX1 |
| Water Capacity | 680 L | Air Blower Pump | 400W/700WX1 |
|  |  |  |  |
| **Jets Configuration** |  | **Other Equipments** |  |
| Total jets | 83 PCS | Spa Top Hard Cover | 1 PCS |
| Water jets (3.5") | 3 PCS | Insulation Foam For Shell | 1 PCS |
| Water jets (2") | 60 PCS | Pine Wood Skirt Step | 1 SET |
| Air jets | 20 PCS | Water Fountains | 1 PCS |
|  |  | Ozone & Filter | 1 PCS |
|  |  | LED Light (5") | 1 PCS |
|  |  | Small LED Light | 18 PCS |
|  |  | Surface Valves | 1 SET |
|  |  | Suction | 3 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
| **[PoolTech-58](https://pooltech.dk/produkt/pooltech-58/)** |  | **Electric components** |  |
| Size | 2000x2000x910 mm | Control System | 1 SET |
| Seat | 5 Person (two louge) | Heater | 1X3KW |
| Material | US Acrylic | Whirlpool Pump | 3HPX1 |
| Gross weight | 300 KG | Circulate Pump | 1HP/0.35HPX1 |
| Water Capacity | 900 L | Air Blower Pump | 400W/700WX1 |
|  |  |  |  |
| **Jets Configuration** |  | **Other Equipments** |  |
| Total jets | 60 PCS | Spa Top Hard Cover | 1 PCS |
| Single rotating jets (5") | 2 PCS | Insulation Foam For Shell | 1 PCS |
| Single rotating jets (3") | 2 PCS | Pine Wood Skirt Step | 1 SET |
| Making surf jets (5") | 1 PCS | Water Fountains | 3 PCS |
| Dual rotating jets (5") | 2 PCS | Ozone & Filter | 1 PCS |
| Water jets (5") | 3 PCS | LED Light (5") | 1 PCS |
| Water jets (3") | 4 PCS | LED Light | 24 PCS |
| Water jets (2") | 32 PCS | Surface Valves | 1 SET |
| Air jets | 14 PCS | Suction | 2 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
| **[PoolTech-67](https://pooltech.dk/produkt/pooltech-67/)** |  | Electric components |  |
| Size | 2400x2400x950 mm | Control System | 1 SET |
| Seat | 6-7 Person | Heater | 1X3KW |
| Material | US Acrylic | Whirlpool Pump | 2HPX2 |
| Gross weight | 480 KG | Circulate Pump | 1HP/0.35HPX1 |
| Water Capacity | 1700 L | Air Blower Pump | 400W/700WX1 |
|  |  |  |  |
| Jets Configuration |  | Other Equipments |  |
| Total jets | 65 PCS | Spa Top Hard Cover | 1 PCS |
| Rotating therapy jets (5") | 1 PCS | Insulation Foam For Shell | 1 PCS |
| Rotating therapy jets (4") | 4 PCS | Pine Wood Skirt Step | 1 SET |
| Water jets (4") | 10 PCS | Water fountain | 2 PCS |
| Water jets (2") | 32 PCS | Ozone & Filter | 1 PCS |
| Air jets | 18 PCS | Underwater LED Light | 1 PCS |
|  |  | LED Light | 14 PCS |
|  |  | Surface Valves | 1 SET |
|  |  | Suction | 3 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
| **[PoolTech-18](https://pooltech.dk/produkt/pooltech-18/)** |  | **Electric components** |  |
| Size | 2400x2400x1000 mm | Control System | 1 SET |
| Seat | 6-7 Person (one louge) | Heater | 1X3KW |
| Material | US Acrylic | Whirlpool Pump | 3HPX1/2HPX2 |
| Gross weight | 500 KG | Circulate Pump | 1HP/0.35HPX1 |
| Water Capacity | 1690 L | Air Blower Pump | 400W/700WX1 |
|  |  |  |  |
| **Jets Configuration** |  | **Other Equipments** |  |
| Total jets | 126 PCS | Spa Top Hard Cover | 1 PCS |
| Water therapy jets (2.5") | 33 PCS | Insulation Foam For Shell | 1 PCS |
| Water jets (2") | 73 PCS | Pine Wood Skirt Step | 1 SET |
| Air jets | 16 PCS | Fountains | 2 PCS |
| Surfing jets (5") | 1 PCS | Ozone & Filter | 1 PCS |
| Rotating therapy jets (5") | 3 PCS | Underwater LED Light (5") | 1 PCS |
|  |  | LED Light | 15 PCS |
|  |  | Surface Valves | 1 SET |
|  |  | Suction | 4 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
| **[PoolTech-88](https://pooltech.dk/produkt/pooltech-88/)** |  | **Electric components** |  |
| Size | 2400x2400x930 mm | Control System | 1 SET |
| Seat | 7-8 Person | Heater | 1X3KW |
| Material | US Acrylic | Whirlpool Pump | 3HPX1/2HPX1 |
| Gross weight | 480 KG | Circulate Pump | 0.35HPX2 |
| Water Capacity | 600 L | Air Blower Pump | 400W/700WX1 |
|  |  |  |  |
| Jets Configuration |  | Other Equipments |  |
| Total jets | 89 PCS | Spa Top Hard Cover | 1 PCS |
| Surfing jet (5") | 1 PCS | Insulation Foam For Shell | 1 PCS |
| Rotating therapy jets (5") | 2 PCS | Pine Wood Skirt Step | 1 SET |
| Rotating therapy jets (3.5") | 9 PCS |  |  |
| Water jets (5") | 2 PCS | Ozone & Filter | 1 PCS |
| Water jets (3.5") | 10 PCS | Underwater LED Light | 1 PCS |
| Water jets (2") | 51 PCS | LED Light | 12 PCS |
| Air jets | 14 PCS | Surface Valves | 1 SET |
|  |  | Suction | 3 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
| [**PoolTech-89**](https://pooltech.dk/produkt/pooltech-89/) |  | **Electric components** |  |
| Size | 2400x2400x930 mm | Control System | 1 SET |
| Seat | 6-7 Person | Heater | 1X3KW |
| Material | US Acrylic | Whirlpool Pump | 3HPX1/2HPX1 |
| Gross weight | 480 KG | Circulate Pump | 0.35HPX2 |
| Water Capacity | 600 L | Air Blower Pump | 400W/700WX1 |
|  |  |  |  |
| **Jets Configuration** |  | **Other Equipments** |  |
| Total jets | 79 PCS | Spa Top Hard Cover | 1 PCS |
| Surfing jet (5") | 1 PCS | Insulation Foam For Shell | 1 PCS |
| Rotating therapy jets (3.5") | 5 PCS | Pine Wood Skirt Step | 1 SET |
| Water jets (5") | 2 PCS |  |  |
| Water jets (3.5") | 10 PCS | Ozone & Filter | 1 PCS |
| Water jets (2") | 45 PCS | Underwater LED Light | 1 PCS |
| Air jets | 16 PCS | LED Light | 12 PCS |
|  |  | Surface Valves | 1 SET |
|  |  | Suction | 4 PCS |
| **[PoolTech-99](https://pooltech.dk/produkt/pooltech-99/)** |  | **Electric components** |  |
| Size | 3800x2400x930 mm | Control System | 1 SET |
| Seat | 13-14 Person | Heater | 1X3KW |
| Material | US Acrylic | Whirlpool Pump | 3HPX1/2HPX2 |
| Gross weight | 1100 KG | Circulate Pump | 0.35HPX2 |
| Water Capacity | 4300 L | Air Blower Pump | 400W/700WX1 |
|  |  |  |  |
| **Jets Configuration** |  | **Other Equipments** |  |
| Total jets | 119 PCS | Spa Top Hard Cover | 1 PCS |
| Rotating therapy jets (3.5") | 10 PCS | Insulation Foam For Shell | 1 PCS |
| Water jets (5") | 2 PCS | Pine Wood Skirt Step | 1 SET |
| Water jets (3.5") | 12 PCS |  |  |
| Water jets (2") | 69 PCS | Ozone & Filter | 1 PCS |
| Air jets | 26 PCS | Underwater LED Light | 2 PCS |
|  |  | LED Light | 16 PCS |
|  |  | Surface Valves | 1 SET |
|  |  | Suction | 4 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
| **[PoolTech-08](https://pooltech.dk/produkt/pooltech-08/)** |  | **Electric components** |  |
| Size | 2400x2400x930 mm | Control System | 1 SET |
| Seat | 6-7 Person (two louge) | Heater | 1X3KW |
| Material | US Acrylic | Whirlpool Pump | 3HPX1/2HPX1 |
| Gross weight | 500 KG | Circulate Pump | 1HP/0.35HPX1 |
| Water Capacity | 1650 L | Air Blower Pump | 400W/700WX1 |
|  |  |  |  |
| **Jets Configuration** |  | **Other Equipments** |  |
| Total jets | 102 PCS | Spa Top Hard Cover | 1 PCS |
| Water therapy jets (5") | 1 PCS | Insulation Foam For Shell | 1 PCS |
| Water therapy jets (3.5") | 7 PCS | Pine Wood Skirt Step | 1 SET |
| Water therapy jets (2") | 73 PCS | Waterfall | 1 PCS |
| air jets | 14 PCS | Ozone & Filter | 1 PCS |
| Rotating therapy jets (3.5") | 7 PCS | LED Light (5") | 1 PCS |
|  |  | LED Light (Small) | 45 PCS |
|  |  | Surface Valves | 1 SET |
|  |  | Suction | 3 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
| **[PoolTech-08S](https://pooltech.dk/produkt/pooltech-08s/)** |  | **Electric components** |  |
| Size | 2200x2200x970 mm | Control System | 1 SET |
| Seat | 6 Person (one louge) | Heater | 1X3KW |
| Material | US Acrylic | Whirlpool Pump | 2HPX2 |
| Gross weight | 360 KG | Circulate Pump | 0.35HPX1 |
| Water Capacity | 1400 L | Air Blower Pump | / |
|  |  |  |  |
| **Jets Configuration** |  | **Other Equipments** |  |
| Total jets | 76 PCS | Spa Top Hard Cover | 1 PCS |
| Water therapy jets (5") | 1 PCS | Insulation Foam For Shell | 1 PCS |
| Water therapy jets (3.5") | 11 PCS | Pine Wood Skirt Step | 1 SET |
| Water therapy jets (2") | 58 PCS | Waterfall | 1 PCS |
| Rotating jets (3.5") | 6 PCS | Ozone & Filter | 1 PCS |
|  |  | LED Light (5") | 1 PCS |
|  |  | LED Light (Small) | 31 PCS |
|  |  | Surface Valves | 1 SET |
|  |  | Suction | 3 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
| **[PoolTech-09](https://pooltech.dk/produkt/pooltech-09/)** |  | **Electric components** |  |
| Size | 2200x2200x970 mm | Control System | 1 SET |
| Seat | 7 Person (one louge) | Heater | 1X3KW |
| Material | US Acrylic | Whirlpool Pump | 3HPX1/2HPX1 |
| Gross weight | 400 KG | Circulate Pump | 0.35HPX1 |
| Water Capacity | 1400 L | Air Blower Pump | 400WX1 |
|  |  |  |  |
| **Jets Configuration** |  | **Other Equipments** |  |
| Total jets | 109 PCS | Spa Top Hard Cover | 1 PCS |
| Water therapy jets (5") | 2 PCS | Insulation Foam For Shell | 1 PCS |
| Water therapy jets (3.5") | 5 PCS | Pine Wood Skirt Step | 1 SET |
| Water jets (2") | 83 PCS | Fountain | 2 PCS |
| air jets | 14 PCS | Ozone & Filter | 1 PCS |
| Water Rotating jets (3.5") | 4 PCS | LED Light (5") | 1 PCS |
|  |  | LED Light (Small) | 48 PCS |
|  |  | Surface Valves | 1 SET |
|  |  | Suction | 3 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
| **[PoolTech-09S](https://pooltech.dk/produkt/pooltech-09s/)** |  | **Electric components** |  |
| Size | 2200x2200x970 mm | Control System | 1 SET |
| Seat | 7 Person (one louge) | Heater | 1X3KW |
| Material | US Acrylic | Whirlpool Pump | 2HPX2 |
| Gross weight | 360 KG | Circulate Pump | 0.35HPX1 |
| Water Capacity | 1400 L | Air Blower Pump | / |
|  |  |  |  |
| **Jets Configuration** |  | **Other Equipments** |  |
| Total jets | 68 PCS | Spa Top Hard Cover | 1 PCS |
| Water therapy jets (5") | 3 PCS | Insulation Foam For Shell | 1 PCS |
| Water therapy jets (3.5") | 9 PCS | Pine Wood Skirt Step | 1 SET |
| Water therapy jets (2") | 50 PCS | Fountain | 1 PCS |
| Rotating jets (3.5") | 6 PCS | Ozone & Filter | 1 PCS |
|  |  | LED Light (5") | 1 PCS |
|  |  | LED Light (Small) | 34 PCS |
|  |  | Surface Valves | 1 SET |
|  |  | Suction | 3 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
| **[PoolTech-12](https://pooltech.dk/produkt/pooltech-12/)** |  | **Electric components** |  |
| Size | 2200x2200x970 mm | Control System | 1 SET |
| Seat | 5 Person | Heater | 1X3KW |
| Material | US Acrylic | Whirlpool Pump | 3HPX1/2HPX1 |
| Gross weight | 400 KG | Circulate Pump | 1HP/0.35HPX1 |
| Water Capacity | 1400 L | Air Blower Pump | 400W/700WX1 |
|  |  |  |  |
| **Jets Configuration** |  | **Other Equipments** |  |
| Total jets | 102 PCS | Spa Top Hard Cover | 1 PCS |
| Water therapy jets (5") | 3 PCS | Insulation Foam For Shell | 1 PCS |
| Water therapy jets (3.5") | 10 PCS | Pine Wood Skirt Step | 1 SET |
| Water therapy jets (2") | 49 PCS | Fountain | 1 PCS |
| Rotating therapy jets (3.5") | 8 PCS | Ozone & Filter | 1 PCS |
|  |  | LED Light (5") | 1 PCS |
|  |  | LED Light (Small) | 42 PCS |
|  |  | Surface Valves | 1 SET |
|  |  | Suction | 3 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
| **[PoolTech-12S](https://pooltech.dk/produkt/pooltech-12s/)** |  | **Electric components** |  |
| Size | 2200x2200x970 mm | Control System | 1 SET |
| Seat | 5 Person | Heater | 1X3KW |
| Material | US Acrylic | Whirlpool Pump | 2HPX2 |
| Gross weight | 400 KG | Circulate Pump | 0.35HPX1 |
| Water Capacity | 1400 L | Air Blower Pump | / |
|  |  |  |  |
| **Jets Configuration** |  | **Other Equipments** |  |
| Total jets | 70 PCS | Spa Top Hard Cover | 1 PCS |
| Water therapy jets (5") | 3 PCS | Insulation Foam For Shell | 1 PCS |
| Water therapy jets (3.5") | 10 PCS | Pine Wood Skirt Step | 1 SET |
| Water therapy jets (2") | 49 PCS | Fountain | 3 PCS |
| Rotating jets (3.5") | 8 PCS | Ozone & Filter | 1 PCS |
|  |  | LED Light (5") | 1 PCS |
|  |  | LED Light (Small) | 42 PCS |
|  |  | Surface Valves | 1 SET |
|  |  | Suction | 3 PCS |
|  |  | Waterfall | 1 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
| **[PoolTech-13](https://pooltech.dk/produkt/pooltech-13/)** |  | **Electric components** |  |
| Size | 2100x1500x820 mm | Control System | 1 SET |
| Seat | 3 Person | Heater | 1X3KW |
| Material | US Acrylic | Whirlpool Pump | 3HPX1 |
| Gross weight | 250 KG | Circulate Pump | 0.35HPX1 |
| Water Capacity | 650 L | Air Blower Pump | 400WX1 |
|  |  |  |  |
| **Jets Configuration** |  | **Other Equipments** |  |
| Total jets | 39 PCS | Spa Top Hard Cover | 1 PCS |
| Water therapy jets (5") | 1 PCS | Insulation Foam For Shell | 1 PCS |
| Water therapy jets (3.5") | 2 PCS | Pine Wood Skirt Step | 1 SET |
| Water therapy jets (2") | 24 PCS | Waterfall | 1 PCS |
| Roating therapy Jets (3.5") | 2 PCS | Ozone & Filter | 1 PCS |
| Air jets | 10 PCS | LED Light (5") | 1 PCS |
|  |  | LED Light (Small) | 31 PCS |
|  |  | Surface Valves | 1 SET |
|  |  | Suction | 2 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
| **[PoolTech-61](https://pooltech.dk/produkt/pooltech-61/)** |  | **Electric components** |  |
| Size | 2100x1700x870 mm | Control System | 1 SET |
| Seat | 3 Person | Heater | 1X3KW |
| Material | US Acrylic | Whirlpool Pump | 3HPX1 |
| Gross weight | 300 KG | Circulate Pump | 1HP/0.35HPX1 |
| Water Capacity | 600 L | Air Blower Pump | 400W/700WX1 |
|  |  |  |  |
| **Jets Configuration** |  | **Other Equipments** |  |
| Total jets | 41 PCS | Spa Top Hard Cover | 1 PCS |
| Rotating therapy jets (5") | 1 PCS | Insulation Foam For Shell | 1 PCS |
| Rotating therapy jets (4.5") | 2 PCS | Pine Wood Skirt Step | 1 SET |
| Rotating therapy jets (3.5") | 4 PCS | Waterfall | 1 PCS |
| Water jets (3.5") | 10 PCS | Ozone & Filter | 1 PCS |
| Water jets (2.5") | 17 PCS | LED Light (5") | 1 PCS |
| Air jets | 6 PCS | LED Light | 16 PCS |
|  |  | Surface Valves | 1 SET |
|  |  | Suction | 2 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
| **[PoolTech-62](https://pooltech.dk/produkt/pooltech-62/)** |  | **Electric components** |  |
| Size | 2200x2200x930 mm | Control System | 1 SET |
| Seat | 5 Person (one louge) | Heater | 1X3KW |
| Material | US Acrylic | Whirlpool Pump | 3HPX1/2HPX1 |
| Gross weight | 400 KG | Circulate Pump | 1HP/0.35HPX1 |
| Water Capacity | 1340 L | Air Blower Pump | 400W/700WX1 |
|  |  |  |  |
| **Jets Configuration** |  | **Other Equipments** |  |
| Total jets | 57 PCS | Spa Top Hard Cover | 1 PCS |
| Big Surfing jets (8") | 1 PCS | Insulation Foam For Shell | 1 PCS |
| Rotating therapy jets (5") | 1 PCS | Pine Wood Skirt Step | 1 SET |
| Rotating therapy jets (4.5") | 6 PCS | Fountains | / |
| Water jets (5") | 2 PCS | Ozone & Filter | 1 PCS |
| Water jets (4.5") | 2 PCS | Underwater LED Light (5") | 1 PCS |
| Water jets (3.5") | 19 PCS | LED Light | 28 PCS |
| Water jets (2.5") | 12 PCS | Surface Valves | 1 SET |
| Water jets (2") | 2 PCS | Suction | 3 PCS |
| Air jets | 10 PCS | Waterfall | 1 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
| **[PoolTech-62A](https://pooltech.dk/produkt/pooltech-62a/)** |  | **Electric components** |  |
| Size | 2200x2200x930 mm | Control System | 1 SET |
| Seat | 5 Person (one louge) | Heater | 1X3KW |
| Material | US Acrylic | Whirlpool Pump | 3HPX11 |
| Gross weight | 400 KG | Circulate Pump | 1HP/0.35HPX1 |
| Water Capacity | 1340 L | Air Blower Pump | 400W/700WX1 |
|  |  |  |  |
| **Jets Configuration** |  | **Other Equipments** |  |
| Total jets | 42 PCS | Spa Top Hard Cover | 1 PCS |
| Rotating therapy jets (5") | 1 PCS | Insulation Foam For Shell | 1 PCS |
| Rotating therapy jets (3.5") | 2 PCS | Pine Wood Skirt Step | 1 SET |
| Water jets (4.5") | 9 PCS | Fountains | / |
| Water jets (3.5") | 9 PCS | Ozone & Filter | 1 PCS |
| Water jets (2.5") | 11 PCS | Underwater LED Light (5") | 1 PCS |
| Air jets | 10 PCS | LED Light | 21 PCS |
|  |  | Surface Valves | 1 SET |
|  |  | Suction | 2 PCS |
|  |  | Waterfall | 1 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
| [**PoolTech-63**](https://pooltech.dk/produkt/pooltech-63/) |  | **Electric components** |  |
| Size | 2200x2200x930 mm | Control System | 1 SET |
| Seat | 6 Person (one louge) | Heater | 1X3KW |
| Material | US Acrylic | Whirlpool Pump | 3HPX1/2HPX1 |
| Gross weight | 400 KG | Circulate Pump | 1HP/0.35HPX1 |
| Water Capacity | 1380 L | Air Blower Pump | 400W/700WX1 |
|  |  |  |  |
| **Jets Configuration** |  | **Other Equipments** |  |
| Total jets | 60 PCS | Spa Top Hard Cover | 1 PCS |
| Big Surfing jets (8") | 1 PCS | Insulation Foam For Shell | 1 PCS |
| Rotating therapy jets (4.5") | 4 PCS | Pine Wood Skirt Step | 1 SET |
| Rotating therapy jets (3.5") | 2 PCS | Waterfall | 2 PCS |
| Water jets (5") | 2 PCS | Ozone & Filter | 1 PCS |
| Water jets (4.5") | 8 PCS | Underwater LED Light (5") | 1 PCS |
| Water jets (3.5") | 11 PCS | LED Light | 21 PCS |
| Water jets (2.5") | 20 PCS | Surface Valves | 1 SET |
| Air jets | 12 PCS | Suction | 3 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
| [**PoolTech-65**](https://pooltech.dk/produkt/pooltech-65/) |  | **Electric components** |  |
| Size | 2300x2300x930 mm | Control System | 1 SET |
| Seat | 5 Person (two louge) | Heater | 1X3KW |
| Material | US Acrylic | Whirlpool Pump | 3HPX2/2HPX1 |
| Gross weight | 450 KG | Circulate Pump | 1HP/0.35HPX1 |
| Water Capacity | 1450 L | Air Blower Pump | 400W/700WX1 |
|  |  |  |  |
| **Jets Configuration** |  | **Other Equipments** |  |
| Total jets | 106 PCS | Spa Top Hard Cover | 1 PCS |
| Rotating therapy jets (5") | 6 PCS | Insulation Foam For Shell | 1 PCS |
| Rotating therapy jets (2.5") | 4 PCS | Pine Wood Skirt Step | 1 SET |
| Water jets (5") | 2 PCS | Waterfall | 1 PCS |
| Water jets (4") | 8 PCS | Ozone & Filter | 1 PCS |
| Water jets (3.5") | 33 PCS | Underwater LED Light (5") | 1 PCS |
| Water jets (2.5") | 2 PCS | LED Light | 19 PCS |
| Water jets (2") | 37 PCS | Surface Valves | 1 SET |
| Air jets | 14 PCS | Suction | 4 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
| **[PoolTech-66](https://pooltech.dk/produkt/pooltech-66/)** |  | **Electric components** |  |
| Size | 2400x2400x930 mm | Control System | 1 SET |
| Seat | 6-7 Person (two louge) | Heater | 1X3KW |
| Material | US Acrylic | Whirlpool Pump | 3HPX2/2HPX1 |
| Gross weight | 500 KG | Circulate Pump | 1HP/0.35HPX1 |
| Water Capacity | 1650 L | Air Blower Pump | 400W/700WX1 |
|  |  |  |  |
| **Jets Configuration** |  | **Other Equipments** |  |
| Total jets | 123 PCS | Spa Top Hard Cover | 1 PCS |
| Large surfing jets (7") | 3 PCS | Insulation Foam For Shell | 1 PCS |
| Rotating therapy jets (5") | 2 PCS | Pine Wood Skirt Step | 1 SET |
| Rotating therapy jets (4") | 6 PCS | Water fountain | 3 PCS |
| Rotating therapy jets (2.5") | 2 PCS | Ozone & Filter | 1 PCS |
| Water jets (4") | 13 PCS | Underwater LED Light | 1 PCS |
| Water jets (3") | 4 PCS | LED Light | 30 PCS |
| Water jets (2.5") | 39 PCS | Surface Valves | 1 SET |
| Water jets (2") | 40 PCS | Suction | 5 PCS |
| Air jets | 14 PCS |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **[PoolTech-21](https://pooltech.dk/produkt/pooltech-21/)** |  | **Electric components** |  |
| Size | 1800x1300x840 mm | Control System | 1 SET |
| Seat | 2-3 Person | Heater | 1X3KW |
| Material | US Acrylic | Whirlpool Pump | 2HPX1 |
| Gross weight | 260 KG | Circulate Pump | 1HP/0.35HPX1 |
| Water Capacity | 510 L | Air Blower Pump | 400W/700WX1 |
|  |  |  |  |
| **Jets Configuration** |  | **Other Equipments** |  |
| Total jets | 39 PCS | Spa Top Hard Cover | 1 PCS |
| Hydro therapy water jets (2.5") | 15 PCS | Insulation Foam For Shell | 1 PCS |
| Water jets (2") | 13 PCS | Pine Wood Skirt Step | 1 SET |
| Air jets | 11 PCS | Drainage | 1 PCS |
|  |  | Ozone & Filter | 1 PCS |
|  |  | LED Light (5") | 1 PCS |
|  |  | LED Light (2") | 8 PCS |
|  |  | Surface Valves | 1 SET |
|  |  | Suction | 1 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
| **[PoolTech-16A](https://pooltech.dk/produkt/pooltech-16a/)** |  | **Electric components** |  |
| Size | 2400x2400x930 mm | Control System | 1 SET |
| Seat | 6-7 Person (two louge) | Heater | 1X3KW |
| Material | US Acrylic | Whirlpool Pump | 3HPX1/2HPX2 |
| Gross weight | 500 KG | Circulate Pump | 1HP/0.35HPX1 |
| Water Capacity | 1650 L | Air Blower Pump | 400W/700WX1 |
|  |  |  |  |
| **Jets Configuration** |  | **Other Equipments** |  |
| Total jets | 163 PCS | Spa Top Hard Cover | 1 PCS |
| Water jets (5") | 2 PCS | Insulation Foam For Shell | 1 PCS |
| Water jets (4") | 7 PCS | Pine Wood Skirt Step | 1 SET |
| Water jets (3") | 6 PCS | Fountains | 2 PCS |
| Water jets (2") | 115 PCS | Ozone & Filter | 1 PCS |
| Rotating therapy jets (3") | 8 PCS | Underwater LED Light (5") | 1 PCS |
| Surfing jets (5") | 1 PCS | LED Light | 20 PCS |
| Air jets | 22 PCS | Surface Valves | 1 SET |
| Shoulder massage jets | 2 PCS | Suction | 5 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
| **[PoolTech-17](https://pooltech.dk/produkt/pooltech-17/)** |  | **Electric components** |  |
| Size | 2200x2200x930 mm | Control System | 1 SET |
| Seat | 5 Person (two louge) | Heater | 1X3KW |
| Material | US Acrylic | Whirlpool Pump | 3HPX1/2HPX1 |
| Gross weight | 390 KG | Circulate Pump | 1HP/0.35HPX1 |
| Water Capacity | 1600 L | Air Blower Pump | 400W/700WX1 |
|  |  |  |  |
| **Jets Configuration** |  | **Other Equipments** |  |
| Total jets | 67 PCS | Spa Top Hard Cover | 1 PCS |
| Water jets (3.5") | 16 PCS | Insulation Foam For Shell | 1 PCS |
| Water jets (2") | 32 PCS | Pine Wood Skirt Step | 1 SET |
| Air jets | 12 PCS | Fountains | 1 PCS |
| Surfing jets (5") | 1 PCS | Ozone & Filter | 1 PCS |
| Rotating therapy jets (5") | 2 PCS | Underwater LED Light | 1 PCS |
| Rotating therapy jets (4") | 4 PCS | LED Light | 15 PCS |
|  |  | Surface Valves | 1 SET |
|  |  | Suction | 4 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
| **[PoolTech-27](https://pooltech.dk/produkt/pooltech-27/)** |  | **Electric components** |  |
| Size | 2100x1600x870 mm | Control System | 1 SET |
| Seat | 3 Person (two louge) | Heater | 1X3KW |
| Material | US Acrylic | Whirlpool Pump | 3HPX1 |
| Gross weight | 300 KG | Circulate Pump | 1HP/0.35HPX1 |
| Water Capacity | 600 L | Air Blower Pump | 400W/700WX1 |
|  |  |  |  |
| **Jets Configuration** |  | **Other Equipments** |  |
| Total jets | 40 PCS | Spa Top Hard Cover | 1 PCS |
| Water jets (5") | 2 PCS | Insulation Foam For Shell | 1 PCS |
| Water jets (2") | 16 PCS | Pine Wood Skirt Step | 1 SET |
| Air jets | 8 PCS | Fountains | / |
| Rotating therapy jets (4") | 4 PCS | Ozone & Filter | 1 PCS |
| Hydrotherapy jets (3.5") | 10 PCS | LED Light (5") | 1 PCS |
|  |  | LED Light | 13 PCS |
|  |  | Surface Valves | 1 SET |
|  |  | Suction | 3 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
| **[PoolTech-37](https://pooltech.dk/produkt/pooltech-37/)** |  | **Electric components** |  |
| Size | 2200x2200x930 mm | Control System | 1 SET |
| Seat | 5 Person | Heater | 1X3KW |
| Material | US Acrylic | Whirlpool Pump | 3HPX1 |
| Gross weight | 410 KG | Circulate Pump | 1HP/0.35HPX1 |
| Water Capacity | 1350 L | Air Blower Pump | 400W/700WX1 |
|  |  |  |  |
| **Jets Configuration** |  | **Other Equipments** |  |
| Total jets | 72 PCS | Spa Top Hard Cover | 1 PCS |
| Water jets (5") | 1 PCS | Insulation Foam For Shell | 1 PCS |
| Water jets (4") | 8 PCS | Pine Wood Skirt Step | 1 SET |
| Air jets | 16 PCS | Water Fountains | 2 PCS |
| Water jets (2") | 33 PCS | Ozone & Filter | 1 PCS |
| Rotating therapy jets (4") | 8 PCS | LED Light (5") | 1 PCS |
| Rotating therapy jets (2.5") | 6 PCS | LED Light | 18 PCS |
|  |  | Surface Valves | 1 SET |
|  |  | Suction | 3 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
| **[PoolTech-57](https://pooltech.dk/produkt/pooltech-57/)** |  | **Electric components** |  |
| Size | 1950x1950x930 mm | Control System | 1 SET |
| Seat | 4-6 Person | Heater | 1X3KW |
| Material | US Acrylic | Whirlpool Pump | 3HPX1 |
| Gross weight | 280 KG | Circulate Pump | 1HP/0.35HPX1 |
| Water Capacity | 900 L | Air Blower Pump | 400W/700WX1 |
|  |  |  |  |
| **Jets Configuration** |  | **Other Equipments** |  |
| Total jets | 36 PCS | Spa Top Hard Cover | 1 PCS |
| Rotating therapy jets (5") | 1 PCS | Insulation Foam For Shell | 1 PCS |
| Rotating therapy jets (4") | 2 PCS | Pine Wood Skirt Step | 1 SET |
| Water jets (4") | 6 PCS | Fountains | 2 PCS |
| Water jets (3.5") | 2 PCS | Ozone & Filter | 1 PCS |
| Water jets (2") | 17 PCS | LED Light (5") | 1 PCS |
| Air jets | 8 PCS | LED Light | 15 PCS |
|  |  | Surface Valves | 1 SET |
|  |  | Suction | 3 PCS |
|  |  | Waterfall | 1 PCS |

|  |  |  |  |
| --- | --- | --- | --- |
| **[PoolTech-57A](https://pooltech.dk/produkt/pooltech-57a/)** |  | **Electric components** |  |
| Size | 1950x1950x930 mm | Control System | 1 SET |
| Seat | 5 Person (one louge) | Heater | 1X3KW |
| Material | US Acrylic | Whirlpool Pump | 3HPX1 |
| Gross weight | 290 KG | Circulate Pump | 1HP/0.35HPX1 |
| Water Capacity | 950 L | Air Blower Pump | 400W/700WX1 |
|  |  |  |  |
| **Jets Configuration** |  | **Other Equipments** |  |
| Total jets | 40 PCS | Spa Top Hard Cover | 1 PCS |
| Surfing therapy jets (5") | 1 PCS | Insulation Foam For Shell | 1 PCS |
| Hydro therapy jets (5") | 2 PCS | Pine Wood Skirt Step | 1 SET |
| Hydro therapy jets (4") | 1 PCS | Fountains | 2 PCS |
| Hydro therapy jets (3.5") | 8 PCS | Ozone & Filter | 1 PCS |
| Hydro therapy jets (2") | 20 PCS | LED Light (5") | 1 PCS |
| Air jets (1.5") | 8 PCS | LED Light | 18 PCS |
|  |  | Surface Valves | 1 SET |
|  |  | Suction | 2 PCS |